Koala Kare Products

Approved Copy Points for Distributors

KB200

* Koala Polypropylene surface mounted horizontal baby changing station.
* Unibody steel chassis supports 200 lbs with minimal deflection.
* Sleek design matches modern restroom design and décor.
* Available in four colors.
* Steel on steel hinge has greater resistance to wear and improved durability.
* Gas spring mechanism ensures smooth open and close.
* Dual liner cavity with lock minimizes operator refills and discourages potential vandalism.
* Includes child protection straps and bag hooks.
* Fully ASTM and EN compliant. TUV Certification. Meets all ADA requirements.
* Bed surface exclusively contains Microban® antimicrobial, reducing odor causing bacteria.
* Constructed with 16% recycled materials; contributes to LEED certified building requirements.

Dimensions: 35 3/16” W x 22¼” H (894 mm W x 565 mm H)

Depth Closed: 4” (102 mm)

Depth Open: 23 3/16” (589 mm)

Colors: Cream (00), Grey (01), White Granite (05), Earth (11)

You may also use the most current version of the technical data sheet..